**MAN E3872LE**

Original BOSCH® knock sensors, 2 per engine bank.

The following sensor inputs at DetCon20 need to be bridged

English:

|  |  |  |
| --- | --- | --- |
| **Firing order** | **Sensor input DetCon** | **Bridge inputs** |
|  | 1 |  |
|  | 2 |  |
|  | 3 |  |
|  | 4 |  |
|  | 5 |  |
|  | 6 |  |
|  | 7 |  |
|  | 8 |  |
|  | 9 |  |
|  | 10 |  |
|  | 11 |  |
|  | 12 |  |